=====================================================================  
MSP     TITLE                                   DOWN STATUS CRITERIA  
CODE  
=====================================================================  
014     FCCA TERMINAL FAIL                      SINGLE OCCURRENCE  
015     FCCB TERMINAL FAIL                      SINGLE OCCURRENCE  
187\*    ACCELEROMETER SENSOR A FAIL             SINGLE OCCURRENCE  
188\*    ACCELEROMETER SENSOR B FAIL             SINGLE OCCURRENCE  
193\*    RUDDER CONTROL FAILED                   SINGLE OCCURRENCE  
194\*    FCS CONTROL PANEL FAIL                  SINGLE OCCURRENCE  
195\*    READ BLIN CODES                         SINGLE OCCURRENCE  
196\*    LEFT PRESSURE TRANSMITTER SET FAIL      SINGLE OCCURRENCE  
197\*    RIGHT PRESSURE TRANSMITTER SET FAIL     SINGLE OCCURRENCE  
198\*    LEFT TOTAL TEMPERATURE PROBE FAIL       SINGLE OCCURRENCE  
199\*    RIGHT TOTAL TEMPERATURE PROBE FAIL      SINGLE OCCURRENCE  
200\*    BARO SET FAIL                           SINGLE OCCURRENCE  
201\*    FCS CABLE FAIL, FCS CONTROL PANEL,      SINGLE OCCURRENCE  
       FCCA  
202\*    FCS CABLE FAIL, FCS CONTROL PANEL,      SINGLE OCCURRENCE  
       FCCB  
203\*    FCS CABLE FAIL, STICK GRIP              SINGLE OCCURRENCE  
204\*    FCS CABLE FAIL, STICK POSITION SENSORS  SINGLE OCCURRENCE  
205\*    FCS CABLE FAIL, RUDDER CONTROL, FCCA    SINGLE OCCURRENCE  
  
206\*    FCS CABLE FAIL, RUDDER CONTROL, FCCB    SINGLE OCCURRENCE  
207\*    FCS CABLE FAIL, REAR RUDDER CONTROL,    SINGLE OCCURRENCE  
       FCCA  
208\*    FCS CABLE FAIL, REAR RUDDER CONTROL,    SINGLE OCCURRENCE  
       FCCB  
211\*    FCS CABLE FAIL, ACCELEROMETER, FCCA     SINGLE OCCURRENCE  
212\*    FCS CABLE FAIL, ACCELEROMETER, FCCB     SINGLE OCCURRENCE  
213\*    FCS CABLE FAIL, RATE GYROSCOPE/AHRS,    SINGLE OCCURRENCE  
       FCCA  
214\*    FCS CABLE FAIL, RATE GYROSCOPE/AHRS,    SINGLE OCCURRENCE  
       FCCB  
215\*    FCS CABLE FAIL, NWS POWER UNIT          SINGLE OCCURRENCE  
217\*    MAD FAIL                                SINGLE OCCURRENCE  
218\*    RUN NWS MODE OF M-BIT                   SINGLE OCCURRENCE  
22A\*    LEFT LEF HDU FAIL                       SINGLE OCCURRENCE  
22C\*    RIGHT LEF HDU FAIL                      SINGLE OCCURRENCE  
426     RECCE DOOR DISCRETE FROM FCS FAIL       SINGLE OCCURRENCE  
427     FCC USING INCORRECT SOURCE ERROR        SINGLE OCCURRENCE  
       CORRECTION  
441     L FEED SOV FAIL TO OPEN/CLOSE           SINGLE OCCURRENCE  
442     L BOOST SWITCH FAIL                     SINGLE OCCURRENCE  
443     TANK 2 INTERCONNECT VALVE FAIL          THREE SEPARATE  
                                               OCCURRENCES IN THE  
                                               LAST TEN FLIGHTS  
444     L TURBINE BOOST PUMP FAIL               THREE SEPARATE  
                                               OCCURRENCES IN THE  
                                               LAST TEN FLIGHTS  
445     L MOTIVE BOOST PUMP FAIL                SINGLE OCCURRENCE  
448     R BOOST SWITCH FAIL                     SINGLE OCCURRENCE  
449     TANK 3 INTERCONNECT VALVE FAIL          THREE SEPARATE  
                                               OCCURRENCES IN THE  
                                               LAST TEN FLIGHTS  
450     R TURBINE BOOST PUMP FAIL               THREE SEPARATE  
                                               OCCURRENCES IN THE  
                                               LAST TEN FLIGHTS  
451     R MOTIVE BOOST PUMP FAIL                SINGLE OCCURRENCE  
454     TANK 1 INTERCONNECT VALVE FAIL          THREE SEPARATE  
                                               OCCURRENCES IN THE  
                                               LAST TEN FLIGHTS  
455     TANK 1 INTERCONNECT SOLENOID FAIL       THREE SEPARATE  
                                               OCCURRENCES IN THE  
                                               LAST TEN FLIGHTS  
456     TANK 1 AMBIGUITY                        THREE SEPARATE  
                                               OCCURRENCES IN THE  
                                               LAST TEN FLIGHTS  
459     L WING TRANSFER SOV FAIL TO CLOSE       SINGLE OCCURRENCE OF  
                                               459 AND 511 DURING  
                                               THE SAME FLIGHT  
462     R WING MOTIVE SOV FAIL TO CLOSE         SINGLE OCCURRENCE OF  
                                               462 AND 511 DURING  
                                               THE SAME FLIGHT  
478     TANK 2 TRANSFER SOV FAIL OPEN           SINGLE OCCURRENCE OF  
                                               478 AND 511 DURING  
                                               THE SAME FLIGHT  
479     TANK 2 LEVEL CONTROL VALVE FAIL         SINGLE OCCURRENCE AND  
                                               FUEL LO CAUTION  
                                               DURING THE SAME  
                                               FLIGHT  
                                               OR  
                                               THREE SEPARATE  
                                               OCCURRENCES IN THE  
                                               LAST TEN FLIGHTS  
480     TANK 3 TRANSFER SOV FAIL OPEN           SINGLE OCCURRENCE OF  
                                               480 AND 511 DURING  
                                               THE SAME FLIGHT  
481     TANK 3 LEVEL CONTROL VALVE FAIL         SINGLE OCCURRENCE AND  
                                               FUEL LO CAUTION  
                                               DURING THE SAME  
                                               FLIGHT  
                                               OR  
                                               THREE SEPARATE  
                                               OCCURRENCES IN THE  
                                               LAST TEN FLIGHTS  
483     TANK 1 PUMP FAIL                        SINGLE OCCURRENCE  
484     MANIFOLD LEAK                           SINGLE OCCURRENCE OF  
                                               484 AND 511 DURING  
                                               THE SAME FLIGHT  
485     TANK 4 PUMP FAIL                        SINGLE OCCURRENCE  
486     TANK 1 TRANSFER PUMP FAIL OR FUSELAGE   SINGLE OCCURRENCE OF  
       TRANSFER MANIFOLD LEAK                  486 AND 511 DURING  
                                               THE SAME FLIGHT  
487     TANK 4 TRANSFER PUMP FAIL OR FUSELAGE   SINGLE OCCURRENCE OF  
       TRANSFER MANIFOLD LEAK                  487 AND 511 DURING  
                                               THE SAME FLIGHT  
497     INTERNAL PRESSURE REGULATOR FAIL        SINGLE OCCURRENCE AND  
                                               TK PRES HI CAUTION  
                                               DURING THE SAME  
                                               FLIGHT  
502     TANK 2 JET LEVEL SENSOR FAIL            SINGLE OCCURRENCE AND  
                                               FUEL LO CAUTION  
                                               DURING THE SAME  
                                               FLIGHT  
503     TANK 3 JET LEVEL SENSOR FAIL            SINGLE OCCURRENCE AND  
                                               FUEL LO CAUTION  
                                               DURING THE SAME  
                                               FLIGHT  
506     TANK 3 FUEL LOW BIT FAIL                SINGLE OCCURRENCE  
507     TANK 2 FUEL LOW BIT FAIL                SINGLE OCCURRENCE  
511     VENT TANK WET                           SINGLE OCCURRENCE OF  
                                               511 ACCOMPANIED BY  
                                               ANY OF THE FOLLOWING  
                                               DURING THE SAME  
                                               FLIGHT: 459, 462,  
                                               478, 480, 484, 486,  
                                               487  
517     IFR PROBE FAIL                          SINGLE OCCURRENCE  
518     FEED TANK QUANTITY AND FUEL LOW SYSTEM  SINGLE OCCURRENCE  
       DISAGREE  
527     LEFT FUEL /AIR HEAT EXCHANGER BYPASS    SINGLE OCCURRENCE OF  
       VALVE FAIL                              527 AND 595 DURING THE  
                                               SAME FLIGHT  
                                               OR  
                                               SINGLE OCCURRENCE OF  
                                               527 AND L FUEL INLT  
                                               CAUTION DURING THE  
                                               SAME FLIGHT  
549     VENT TANK WET SENSOR FAIL               THREE SEPARATE  
                                               OCCURRENCES IN THE  
                                               LAST TEN FLIGHTS  
533     TK 2 FUEL QUANT. PROBE FAIL             SINGLE OCCURRENCE  
534     TK 3 FUEL QUANT. PROBE FAIL             SINGLE OCCURRENCE  
550     L MOTIVE BOOST PUMP TRANSDUCER FAIL     THREE SEPARATE  
                                               OCCURRENCES IN THE  
                                               LAST TEN FLIGHTS  
551     R MOTIVE BOOST PUMP TRANSDUCER FAIL     THREE SEPARATE  
                                               OCCURRENCES IN THE  
                                               LAST TEN FLIGHTS  
552     FUSELAGE TRANSFER TRANSDUCER FAIL       THREE SEPARATE  
                                               OCCURRENCES IN THE  
                                               LAST TEN FLIGHTS  
553     VENT TANK PRESSURE TRANSDUCER FAIL      SINGLE OCCURRENCE  
558     L WING MOTIVE TRANSDUCER FAIL           THREE SEPARATE  
                                               OCCURRENCES IN THE  
                                               LAST TEN FLIGHTS  
559     R WING MOTIVE TRANSDUCER FAIL           THREE SEPARATE  
                                               OCCURRENCES IN THE  
                                               LAST TEN FLIGHTS  
561     TANK 2 JLS PRESSURE TRANSDUCER/SW FAIL  SINGLE OCCURRENCE  
562     TANK 3 JLS PRESSURE TRANSDUCER/SW FAIL  SINGLE OCCURRENCE  
592     RIGHT FUEL/AIR HEAT EXCHANGER BYPASS    SINGLE OCCURRENCE OF  
       VALVE FAIL                              592 AND 596 DURING THE  
                                               SAME FLIGHT  
                                               OR  
                                               SINGLE OCCURRENCE OF  
                                               592 AND R FUEL INLT  
                                               CAUTION DURING THE  
                                               SAME FLIGHT  
593     MPCD FUEL/AIR HEAT EXCHANGER BACKUP     SINGLE OCCURRENCE OF  
       CONTROL SYSTEM FAIL                     593 AND 595 DURING THE  
                                               SAME FLIGHT  
                                               OR  
                                               SINGLE OCCURRENCE OF  
                                               593 AND 596 DURING THE  
                                               SAME FLIGHT  
594     SDC FUEL/AIR HEAT EXCHANGER BACKUP      SINGLE OCCURRENCE OF  
       CONTROL SYSTEM FAIL                     594 AND 595 DURING THE  
                                               SAME FLIGHT  
                                               OR  
                                               SINGLE OCCURRENCE OF  
                                               594 AND 596 DURING THE  
                                               SAME FLIGHT  
595     LEFT FUEL/AIR HEAT EXCHANGER FUEL LEAK  SINGLE OCCURRENCE  
       DETECTED  
596     RIGHT FUEL/AIR HEAT EXCHANGER FUEL      SINGLE OCCURRENCE  
       LEAK DETECTED  
597     FUEL CROSS-COOLING VALVE FAIL           SINGLE OCCURRENCE  
5C1     AERIAL REFUEL SURGE REGULATOR FAIL      SINGLE OCCURRENCE  
608     L MAIN FUEL M/V EHSV FAIL               SINGLE OCCURRENCE  
656     L ENGINE VIBRATION ACCELEROMETER FAIL   SINGLE OCCURRENCE  
659     L ENGINE PS3 LINE LEAK FAIL             SINGLE OCCURRENCE  
660     L ENGINE P56 LINE LEAK FAIL             SINGLE OCCURRENCE  
662     L ENGINE OIL PRESSURE TRANSMITTER FAIL  SINGLE OCCURRENCE  
664     L ENGINE CHIP DETECTION CIRCUIT FAIL    SINGLE OCCURRENCE  
672     R ENGINE VIBRATION ACCELEROMETER FAIL   SINGLE OCCURRENCE  
675     R ENGINE PS3 LINE LEAK FAIL             SINGLE OCCURRENCE  
676     R ENGINE P56 LINE LEAK FAIL             SINGLE OCCURRENCE  
678     R ENGINE OIL PRESSURE TRANSMITTER FAIL  SINGLE OCCURRENCE  
680     R ENGINE CHIP DETECTION CIRCUIT FAIL    SINGLE OCCURRENCE  
683     L ENGINE FADEC FAIL                     SINGLE OCCURRENCE  
684     L ENGINE FUEL CONTROL/ENGINE FUEL PUMP  SINGLE OCCURRENCE  
       FAIL  
685     L ENGINE SEVERE STALL DETECTED          SINGLE OCCURRENCE  
       (18E-4NE)  
695     L ENGINE EXCITER FAIL                   SINGLE OCCURRENCE  
6A0     L VEN A8 HYDROMECHANICAL FAIL           SINGLE OCCURRENCE  
6A1     L ENGINE FUEL CONTROL HYDROMECHANICAL   SINGLE OCCURRENCE  
       FAIL  
6A9     L ENGINE MISSING FAN BLADE(S)           SINGLE OCCURRENCE  
6C0     R VEN A8 HYDROMECHANICAL FAIL           SINGLE OCCURRENCE  
6C1     R ENGINE FUEL CONTROL HYDROMECHANICAL   SINGLE OCCURRENCE  
       FAIL  
6C9     R ENGINE MISSING FAN BLADE(S)           SINGLE OCCURRENCE  
6E0     L UNEXPECTED AFTERBURNER LIGHT (ON)     SINGLE OCCURRENCE  
       FAIL  
6F0     R UNEXPECTED AFTERBURNER LIGHT (ON)     SINGLE OCCURRENCE  
       FAIL  
702     L ENGINE LEVEL 3 EGT OVERTEMPERATURE    SINGLE OCCURRENCE  
703     L ENGINE FAN VIBRATION                  SINGLE OCCURRENCE  
704     L ENGINE COMPRESSOR VIBRATION           SINGLE OCCURRENCE  
706     L ENGINE OIL PRESSURE HIGH              SINGLE OCCURRENCE  
707     L ENGINE OIL PRESSURE LOW               SINGLE OCCURRENCE  
709     L ENGINE LEVEL 2 EGT OVERTEMPERATURE    SINGLE OCCURRENCE  
710     L ENGINE LEVEL 3 FAN OVERSPEED          SINGLE OCCURRENCE  
711     L ENGINE LEVEL 2 FAN OVERSPEED          SINGLE OCCURRENCE  
713     L ENGINE LEVEL 3 COMPRESSOR OVERSPEED   SINGLE OCCURRENCE  
714     L ENGINE LEVEL 2 COMPRESSOR OVERSPEED   SINGLE OCCURRENCE  
716     L ENGINE FLAMEOUT                       SINGLE OCCURRENCE  
717     L ENGINE CDP (PS3) OVERPRESSURE         SINGLE OCCURRENCE  
718     L ENGINE STALL                          SINGLE OCCURRENCE  
719     L ENGINE HUNG START                     SINGLE OCCURRENCE  
722     L ENGINE CHIP DETECTED                  SINGLE OCCURRENCE  
733     R ENGINE FADEC FAIL                     SINGLE OCCURRENCE  
734     R ENGINE FUEL CONTROL/ENGINE FUEL PUMP  SINGLE OCCURRENCE  
       FAIL  
735     R ENGINE SEVERE STALL DETECTED          SINGLE OCCURRENCE  
       (18E-4NE)  
745     R ENGINE EXCITER FAIL                   SINGLE OCCURRENCE  
752     R ENGINE LEVEL 3 EGT OVERTEMPERATURE    SINGLE OCCURRENCE  
753     R ENGINE FAN VIBRATION                  SINGLE OCCURRENCE  
754     R ENGINE COMPRESSOR VIBRATION           SINGLE OCCURRENCE  
756     R ENGINE OIL PRESSURE HIGH              SINGLE OCCURRENCE  
757     R ENGINE OIL PRESSURE LOW               SINGLE OCCURRENCE  
759     R ENGINE LEVEL 2 EGT OVERTEMPERATURE    SINGLE OCCURRENCE  
760     R ENGINE LEVEL 3 FAN OVERSPEED          SINGLE OCCURRENCE  
761     R ENGINE LEVEL 2 FAN OVERSPEED          SINGLE OCCURRENCE  
763     R ENGINE LEVEL 3 COMPRESSOR OVERSPEED   SINGLE OCCURRENCE  
764     R ENGINE LEVEL 2 COMPRESSOR OVERSPEED   SINGLE OCCURRENCE  
766     R ENGINE FLAMEOUT                       SINGLE OCCURRENCE  
767     R ENGINE CDP (PS3) OVERPRESSURE         SINGLE OCCURRENCE  
768     R ENGINE STALL                          SINGLE OCCURRENCE  
769     R ENGINE HUNG START                     SINGLE OCCURRENCE  
772     R ENGINE CHIP DETECTED                  SINGLE OCCURRENCE  
791     R MAIN FUEL M/V EHSV FAIL               SINGLE OCCURRENCE  
811     A/C OVERSTRESS (POS EXCEEDANCE)         SINGLE OCCURRENCE  
816     LEFT AMAD OIL PRESSURE LOW              SINGLE OCCURRENCE  
817     RIGHT AMAD OIL PRESSURE LOW             SINGLE OCCURRENCE  
818     LEFT ATSCV OPEN                         THREE SEPARATE  
                                               OCCURRENCES IN THE  
                                               LAST TEN FLIGHTS  
819     RIGHT ATSCV OPEN                        THREE SEPARATE  
                                               OCCURRENCES IN THE  
                                               LAST TEN FLIGHTS  
81A     A/C OVERSTRESS (POS EXCEEDANCE) -       SINGLE OCCURRENCE  
       CATEGORY 2  
81C     A/C OVERSTRESS (POS EXCEEDANCE) -       SINGLE OCCURRENCE  
       DEPOT LEVEL  
833     SECONDARY BLEED AIR OVERPRESSURE        SINGLE OCCURRENCE  
834     LEFT PITOT HEATER CIRCUIT FAIL          SINGLE OCCURRENCE  
835     RIGHT PITOT HEATER CIRCUIT FAIL         SINGLE OCCURRENCE  
848     AVIONICS UNDERCOOL WARN SNSR FAIL       SINGLE OCCURRENCE  
863     AFT COOLING FAN SHUTOFF VLV FAIL        SINGLE OCCURRENCE  
       (ITEM 153)  
874     LEFT FC#1 RELAY FAIL                    SINGLE OCCURRENCE  
875     RIGHT FC#1 RELAY FAIL                   SINGLE OCCURRENCE  
876     LEFT FC#2 RELAY FAIL                    SINGLE OCCURRENCE  
877     RIGHT FC#2 RELAY FAIL                   SINGLE OCCURRENCE  
889     CANOPY SWITCHES DISAGREE                SINGLE OCCURRENCE  
890     RIGHT MLG WEIGHT ON WHEEL SWITCH FAIL   SINGLE OCCURRENCE  
891     LEFT MLG WEIGHT ON WHEEL SWITCH FAIL    SINGLE OCCURRENCE  
892     NLG WEIGHT ON WHEEL SWITCH FAIL         SINGLE OCCURRENCE  
893     RIGHT MLG DOWNLOCK SWITCH FAIL          SINGLE OCCURRENCE  
894     LEFT MLG DOWNLOCK SWITCH FAIL           SINGLE OCCURRENCE  
895     NLG DOWNLOCK SWITCH FAIL                SINGLE OCCURRENCE  
896     RIGHT MLG UPLOCK SWITCH FAIL            SINGLE OCCURRENCE  
897     LEFT MLG UPLOCK SWITCH FAIL             SINGLE OCCURRENCE  
898     NLG UP LOCK SWITCH FAIL                 SINGLE OCCURRENCE  
899     LAUNCH BAR RETRACT PROX SWITCH FAIL     SINGLE OCCURRENCE  
8A0     ECS TERMINAL FAIL                       SINGLE OCCURRENCE  
8A1     ECS CONTROLLER FAIL (ITEM 29)           SINGLE OCCURRENCE  
8A2     L BLEED PRESSURE REGULATOR & SOV FAIL   SINGLE OCCURRENCE  
       (ITEM 1L)  
8A3     R BLEED PRESSURE REGULATOR & SOV FAIL   SINGLE OCCURRENCE  
       (ITEM 1R)  
8A4     AVIONICS FLOW VALVE FAIL (ITEM 8)       SINGLE OCCURRENCE  
8A5     CABIN FLOW VALVE FAIL (ITEM 9)          SINGLE OCCURRENCE  
8A6     SYS FLOW MOD PRESS REGULATING VLV FAIL  SINGLE OCCURRENCE  
       (ITEM 4)  
8A8     CABIN ADD HEAT VALVE FAIL (ITEM 26)     SINGLE OCCURRENCE AND  
                                               AIRCREW REPORT CABIN  
                                               PRESSURIZATION OFF  
                                               SCHEDULE  
                                               OR  
                                               SINGLE OCCURRENCE AND  
                                               AIRCREW REPORT  
                                               INABILITY TO CHANGE  
                                               CABIN TEMPERATURE VIA  
                                               CABIN TEMPERATURE  
                                               KNOB ADJUSTMENT  
8A9     SYS OR AMBIG FAULT - RUN ECS MBIT       SINGLE OCCURRENCE  
       (ITEM SYS)  
8C2     SECONDARY REGULATING AND SHUTOFF VALVE  SINGLE OCCURRENCE  
       FAIL (ITEM 2)  
8C4     RIGHT AUXILIARY SCOOP FAIL (ITEM AXR)   SINGLE OCCURRENCE  
8C5     LEFT AUXILIARY SCOOP FAIL (ITEM AXL)    SINGLE OCCURRENCE  
8C6     ECS AIRCRAFT DISCRETE FAIL (ITEM 15)    SINGLE OCCURRENCE  
8C9     CABIN FLOW SENSOR FAIL (ITEM 175)       SINGLE OCCURRENCE  
8F9     ECS AV VENTURI DELTA P SENS FAIL        SINGLE OCCURRENCE  
       (ITEM 209)  
8FF     ECS ACS CONFIG DISCRETE FAIL            SINGLE OCCURRENCE  
900     LANDING GEAR CONTROL UNIT EMERGENCY     THREE SEPARATE  
       POWER FAIL                              OCCURRENCES IN THE  
                                               LAST TEN FLIGHTS  
901     LEFT MLG PLANING LINK PROXIMITY SWITCH  SINGLE OCCURRENCE  
       FAIL  
902     RIGHT MLG PLANING LINK PROXIMITY        SINGLE OCCURRENCE  
       SWITCH FAIL  
903     HARD LANDING INSPECTION REQUIRED        SINGLE OCCURRENCE  
904     HARD LANDING INSPECTION REQUIRED        SINGLE OCCURRENCE  
910     RIGHT MLG UPLOCK DID NOT OCCUR          SINGLE OCCURRENCE  
911     RIGHT MLG UPLOCK DID NOT OCCUR          SINGLE OCCURRENCE  
912     NLG UPLOCK NOT ACHIEVED                 SINGLE OCCURRENCE  
915     LANDING GEAR CONTROL UNIT FAIL          THREE SEPARATE  
                                               OCCURRENCES IN THE  
                                               LAST TEN FLIGHTS  
916     ARRESTING GEAR DAMPER PRESSURE LOW      SINGLE OCCURRENCE  
925     A/C OVERSTRESS (NEG EXCEEDANCE) -       SINGLE OCCURRENCE  
       CATEGORY 1  
92A     A/C OVERSTRESS (NEG EXCEEDANCE) -       SINGLE OCCURRENCE  
       DEPOT LEVEL  
932     EMERGENCY BRAKE ACCUMULATOR LOW         SINGLE OCCURRENCE  
933     HYD1 RETURN OVERTEMP                    SINGLE OCCURRENCE  
934     HYD2 RETURN OVERTEMP                    SINGLE OCCURRENCE  
935     HYD1 PUMP HOT                           SINGLE OCCURRENCE  
936     HYD2 PUMP HOT                           SINGLE OCCURRENCE  
940     HYD2B PRESSURE REDUCER/SWITCH FAIL      SINGLE OCCURRENCE  
952     BALD CONTROL UNIT FAIL                  SINGLE OCCURRENCE  
953     LEFT ENGINE BALD LOOP LEAK              SINGLE OCCURRENCE  
954     RIGHT ENGINE BALD LOOP LEAK             SINGLE OCCURRENCE  
955     START DUCT BALD LOOP LEAK               SINGLE OCCURRENCE  
956     SECONDARY PRESSURE REGULATOR BALD LOOP  SINGLE OCCURRENCE  
       LEAK  
957     EJECTOR BALD LOOP LEAK                  SINGLE OCCURRENCE  
958     TUNNEL BALD LOOP LEAK                   SINGLE OCCURRENCE  
959     COMPRESSOR DISCHARGE BALD LOOP LEAK     SINGLE OCCURRENCE  
960     PRIMARY HX/INLET BALD LOOP LEAK         SINGLE OCCURRENCE  
961     SECONDARY HX/INLET BALD LOOP LEAK       SINGLE OCCURRENCE  
962     LEFT ENGINE BALD LOOP DETECTOR/CONTROL  SINGLE OCCURRENCE  
       UNIT FAIL  
963     RIGHT ENGINE BALD LOOP DETECTOR/CONTROL SINGLE OCCURRENCE  
       UNIT FAIL  
964     START DUCT BALD LOOP DETECTOR/CONTROL   SINGLE OCCURRENCE  
       UNIT FAIL  
965     SECONDARY PRESS RGLTR BALD LOOP         SINGLE OCCURRENCE  
       DETECTOR/CONTROL UNIT FAIL  
966     EJECTOR BALD LOOP DETECTOR/CONTROL      SINGLE OCCURRENCE  
       UNIT FAIL  
967     TUNNEL BALD LOOP DETECTOR/CONTROL UNIT  SINGLE OCCURRENCE  
       FAIL  
968     COMPRESSOR DISCHARGE BALD LOOP          SINGLE OCCURRENCE  
       DETECTOR/CONTROL UNIT FAIL  
969     PRIMARY HX INLET BALD LOOP DETECTOR/    SINGLE OCCURRENCE  
       CONTROL UNIT FAIL  
970     SECONDARY HX INLET BALD LOOP DETECTOR/  SINGLE OCCURRENCE  
       CONTROL UNIT FAIL  
982     LEFT AMAD OIL LEVEL LOW                 SINGLE OCCURRENCE  
983     RIGHT AMAD OIL LEVEL LOW                SINGLE OCCURRENCE  
985     RLCS LIQUID LEVEL LOW                   SINGLE OCCURRENCE  
999     HYD1/HYD2 OIL LEVEL NOT CHECKED         SINGLE OCCURRENCE  
A30     FIRE EXTINGUISHER LOW                   SINGLE OCCURRENCE  
   C. (\*)MSP CODES WITH AN "\*" HAVE ASSOCIATED BLIN(S) THAT TRIGGER PRIOR  
TO SETTING THE MSP.